==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For Windows NT 4.0 Users
==================================================================
    (c) 1998 Copyright D-Link ALL RIGHTS RESERVED


This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen instructions,
for Windows NT 4.0 users regarding DFE-650 Fast Ethernet PC Card
installation.

Windows NT4.0 users, please also refer to the following.

     -------------------------------------------------------------------
        File              Description/Installation Notes
     -------------------------------------------------------------------
        README.TXT        Overall installation notes for all users

Follow these steps:

     1. Double-click on the "My Computer" icon.
        Then, double-click on the "Control Panel" icon.


     2. In the "Control Panel" window,
        double-click on the "Network" icon.


     3. In the "Network" window,
        Click on the "Adapter".


     4. Click the [Add] button.
        A list of all available drivers will be displayed.

     5. In the "Select Network Adapter" window,
        click on  the [Have Disk...] button, for third-party adapters not
        included in the list, then type a path name to provide a driver.

     6. Insert the DFE-650 Fast Ethernet installation disk into floppy
        disk drive, and type:
              A:\

        Then, Windows NT will attempt to locate the OEMSETUP.INF file in
        the specified path. If it does exists, Windows NT will then copy
        the appropriate drivers to the Windows NT system.


        Till now, the DFE-650 Fast Ethernet drivers are now installed.

        The installation procedure will then proceed to the next steps.
        Please refer to your Windows NT installation guide for information
        on these steps.


        Such steps are:
        Windows NT will pop up one window to ask the value of some
        keywords. Such as  "IO Port", "IRQ Number", "Network Address",
        "Connection Type".

        If you want to change the default MAC Address, USE the
        "Network Address" to specify the MAC Address. The Network Address
        is a 12 digits string(example: 001122334455)


