==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For IPX SHELL Users
==================================================================
    (c) 1998 Copyright D-Link Corporation  ALL RIGHTS RESERVED

This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen instructions,
for IPX SHELL users regarding DFE-650 Fast Ethernet PC Card
installation.


This document contains information on the following topics:

1.0 Introduction
2.0 Installation Notes
___________________________________________________________________


1.0 Introduction
----------------

IPX Shell users please also refer to the following:

    -------------------------------------------------------------------
     File                  Description/Installation notes
    -------------------------------------------------------------------
     \PKTDRV\README.TXT    For all Packet driver users


2.0 Installation Notes
----------------------

There are two methods to run the IPX SHELL program:


Method 1
--------

First, in your CONFIG.SYS file, include the DEVICE command.

  Format:
  DEVICE = DFE650PD.SYS [sw] <packet_int_no> <iobase> <irq> <mem> <S#>

Then, add a DPDIPX statement to your AUTOEXEC.BAT file to load driver
every time you start your computer.


  Example:
  ------------------------
  >DPDIPX
  >NETX
  ><change to last driver>
  >LOGIN <username>



Method 2
--------

Issue DFE650PD command at the DOS command prompt.

  Format:
  DFE650PD [sw] <packet_int_no> <iobase> <irq> <mem> <S#>

  Example:
  ------------------------
  >DFE650PD [sw] <packet_int_no> <iobase> <irq> <mem> <S#>
  >DPDIPX
  >NETX
  ><change to last driver>
  >LOGIN <username>
