==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For All Users
                                                    Version 980701
==================================================================
    (c) 1998 Copyright D-Link Corporation  ALL RIGHTS RESERVED


This document contains general information, which is not included
in the DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen
instructions, for all users regarding DFE-650 Fast Ethernet PC Card
installation.

This document contains information on the following topics:

1.0 What's New?
2.0 Overview
        2.1 About INSTALL.EXE
3.0 To view installation notes and trouble shooting guide
        3.1 Where to find the README file which is specific to your needs
4.0 Version History
5.0 Technical Support Options
        5.1 D-Link Worldwide Web Sites
        5.2 Regional Headquarters

___________________________________________________________________



1.0 What's New?
---------------

The DFE-650 supports the AutoSense, 100BaseTx Half Duplex mode,
10BaseT Full Duplex mode, and 10BaseT Half Duplex mode.

2.0 Overview
------------

The D-Link DFE-650 Fast Ethernet PC Card is designed to work with
notebook or handheld computers that either comes with Socket Services
and Card Serveices or have Intel PC Card controller or compatible
controller.

The ODI DOS driver, NDIS DOS driver, NDIS OS/2 driver, and Windows 95/98
driver are the only network operating system drivers that support an
On-Line Hot-Swap function which allows the card to be removed
and re-inserted without reloading the driver.

After inserting the DFE-650 Fast Ethernet PC Card into a slot,
it is strongly recommended to run INSTALL.EXE in the DOS environment.
Then follow onscreen instructions to complete the installation process.


2.1 About INSTALL.EXE
---------------------

Before running the install.exe, please insert the DFE-650 Fast Ethernet
PC Card into PCMCIA slot in your notebook or handheld computers.  The
install.exe program will find the available resource (IO base address
and Interrupt number) for the DFE-650 Fast Ethernet PC Card automatically.

For the Netware DOS Client users:

    Selecting the "Quick Installation for Netware Client" item of the
    install.exe, installation program will copy the DFE-650 driver to
    the computer and modified the autoexec.bat file of the computer.
    After installation, just restart the computer and will connect
    to the Netware server automatically.

For the other users:

    Running install.exe will display the installation instructions.
    Follow the onscreen instructions to complete the installation
    process.


3.0 To view installation notes
------------------------------


        ============================================
                   Windows '95/98//NT users
        ============================================
For Windows '95/98/NT users, read through this file first then
please view the README.TXT file in each subdirectory.


        ============================================
                          DOS Users
        ============================================
For DOS environment users, including NetWare users, Windows 3.1/3.11
users, firstly read through this file then refer to the INST_DOS.txt
file on the root directory of the DFE-650 Installation Disk for the
installation notes.



3.1 Where to find the README file which is specific to your needs
-----------------------------------------------------------------

 There is one DFE-650 3.5" software diskette.
 And the following two tables give you information about the location and
 contents of the README files that contains information specific to your
 needs.

-------------------------------------------------------------------
File                    Description/Installation notes
--------------------------------------------------------------------
README.TXT              Overall installation notes for all users
INST_DOS.TXT            Overall Installation notes for DOS users,including
                        NetWare users, and Windows 3.1/3.11 users
\NETWARE\README.TXT     Overall installation notes for all NETWARE users
\NETWARE\PCNFS.TXT      Installation notes for PCNFS users
\NETWARE\NW4XX.TXT      Installation notes for NetWare V4.0 or later users
\NETWARE\CLIENT32.TXT   Installation notes for NetWare Client users
\NETWARE\DOSODI.TXT     Installation notes for NetWare DOS Client users
\NETWARE\PRSNLNW.TXT    Installation notes for Personal NetWare users
\NETWARE\NWLITE.TXT     Installation notes for NetWare Lite users
\NETWARE\NW312.TXT      Installation notes for NetWare Server 3.12 users
\DIAG\README.TXT        Notes for Diagnostic Program
\MSLANMAN.DOS\LMDOS.TXT Installation notes for MS LANMAN users
\NDIS2\README.TXT       Overall installation notes for all NDIS users
\NDIS2\MSCLIENT.TXT     Installation notes for MSCLIENT users
\NDIS2\PCNFS.TXT        Installation notes for PCNFS users
\NDIS2\PATHWORK.TXT     Installation notes for PATHWORK users
\NDIS2\PATHWAY.TXT      Installation notes for PATHWAY users
\NDIS2\LANSRV.TXT       Installation notes for IBM Lan Server users
\NDIS2\BANYAN.TXT       Installation notes for Banyan Vines users
\NDIS2\IBMLAN.TXT       Installation notes for IBM DOS Lan users
\PKTDRV\README.TXT      Overall installation notes for all Pcaket Driver users
\PKTDRV\PCTCP.TXT       Installation notes for PCTCP users
\PKTDRV\WINSOCK.TXT     Installation notes for WINSOCK users
\PKTDRV\PDIPX.TXT       Installation notes for IPX users
\PKTDRV\PCNFS.TXT       Installation notes for PC-NFS V5.0 users
\PKTDRV\NCSA.TXT        Installation notes for NCSA users
\WIN95\README.TXT       Installation notes for Windows 95 users
\WIN98\README.TXT       Installation notes for Windows 98 users
\NT351\README.TXT       Installation notes for Windows NT3.51 users
\NT40\README.TXT        Installation notes for Windows NT4.0 users

4.0 Revision History
-----------------------------
Diskette Revision 980701
------------------------
Support Win98 driver

Diskette Revision 980115
------------------------
Modify all drivers to support LXT970's UID.

Revision No:970701
First released driver program


5.0 Technical Support Options
-----------------------------

For technical support information, you may visit D-Link web sites or
contact D-Link authorized dealers, distributors, or the following
D-Link regional headquarters:

     5.1 D-Link Worldwide Web Sites
     ------------------------------

        Information available for all users:

        http:\\www.dlink.com                    U.S.A.
        http:\\www.dlinknet.com                 Canada
        http:\\www.dlink.com.au                 Australia
        http:\\www.dlink.com.cn                 China
        http:\\www.dlink.com.tw                 Asia, Taiwan

     5.2 Regional Headquarters
     -------------------------

        U.S.A.          Web Site:  http:\\www.dlink.com
                        Tel: +1(714)788-0805    Fax: +1(714)753-7033
                        BBS: +1(714)455-1779    BBS: +1(714)455-9616

        Canada          Web Site:  http:\\www.dlinknet.com
                        Tel: +1(905)828-0260    Fax: +1(905)828-5669
                        BBS: +1(965)279-8732

        U.K. & Europe   Tel: +44(181)235-5555   Fax: +44(181)235-5500
                        BBS: +44(181)235-5511

        Germany         Tel: +49(6192)97110     Fax: +49(6192)971111

        Asia, Taiwan    Web Site:  http:\\www.dlink.com.tw
                        Tel: +886(2)916-1600    Fax: +886(2)914-6299
                        BBS: +886(2)910-1835

        France          Tel: +33(1)30238688     Fax: +33(1)30238689

        Sweden          Tel: +46(8)7006211      Fax: +46(8)219640

        Denmark         Tel: +45(43)969040      Fax: +45(43)424347

        Australia       Web Site:  http:\\www.dlink.com.au
                        Tel: +61(2)94177100     Fax: +61(2)94171077
                        BBS: +61(2)94173711

        Singapore       Tel: +657746233         Fax: +657746322
                        BBS: +657744787

        China           Web Site:  http:\\www.dlink.com.cn
                        Tel: +86(10)68467106    Fax: +86(10)68467110

        Tokyo           Tel: +81(3)54349678     Fax: +81(3)54349868

        India           Tel: +91(22)6172478     Fax: +91(22)6172476
                             +91(22)6172479
                             +91(22)6172480


        The BBS communication setup information:
            Speed     :
                2400-14400 baud                          - Germany
                2400-9600  baud                          - Asia, Taiwan
                14400-16800 baud                         - Canada
                9600-14400 baud V32, V32bis, V42, V42bis - U.S.A.
                2400-19200 baud V24, V32, V32bis, V42bis - U.K. & Europe
        Parity    : none
        Data bits : 8
        Stop bit  : 1

_______________________________________________________
All trademarks or tradenames mentioned in this document are
owned by their respective owners.
