==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For NetWare Driver users
==================================================================
    (c) 1998 Copyright D-Link Corporation  ALL RIGHTS RESERVED



This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or on-screen instructions,
for NetWare Driver users regarding DFE-650 Fast Ethernet PC Card
installation.


This document contains information on the following topics:

1.0 Introduction
2.0 Installation Notes
3.0 NET.CFG keywords Available
    3.1 Keyword Definition
___________________________________________________________________



1.0 Introduction
----------------

     The DFE-650 Fast Ethernet PC Card Installation diskette contains
     NetWare driver programs and installation notes for some of the most
     popular operating systems which support NetWare drivers.


2.0 Installation Notes
----------------------

     To view these installation notes, please refer to the following.

    -------------------------------------------------------------------
        File                    Description/Installation Notes
    -------------------------------------------------------------------
      \NETWARE\README.TXT       Overall notes for all NETWARE users
      \NETWARE\PCNFS.TXT        For PCNFS users
      \NETWARE\NW4XX.TXT        For NetWare V4.0 or later users
      \NETWARE\CLIENT32.TXT     For NetWare Client 32 for Windows 95
                                and DOSWIN users
      \NETWARE\DOSODI.TXT       For NetWare Client for DOS users
      \NETWARE\PRSNLNW.TXT      For Personal Netware users
      \NETWARE\NWLITE.TXT       For NetWare Lite users
      \NETWARE\NW312.TXT        For NetWare 3.12 Server users


3.0   NET.CFG Keywords Available
--------------------------------

       This note lists the available NET.CFG keywords for the ODI DOS
       device driver users.

       Most of the keywords are optional and come with default values.
       The available keywords, led by ";", for the NET.CFG file are as
       follows:

                   *** Example NET.CFG file ***
            -------------------------------------------

                Protocol IPX
                         Bind #1

                Link Driver DFE650
        ;            NODE ADDRESS xxxxxxxxxxxx
        ;            PORT 300
        ;            INT 11
                     frame Ethernet_802.3
        ;            frame Ethernet_802.2
        ;            frame Ethernet_II
        ;            frame Ethernet_SNAP

        ;            Protocol IPX 00 Ethernet_802.3
        ;            Protocol IPX E0 Ethernet_802.2
        ;            Protocol IPX 8137 Ethernet_II

3.1  Keyword Definition
-----------------------

        Node Address  -  This keyword specifies the node address
                         (in hexadecimal notation)used by the adapter.
                         This option is used only to override the node
                         address stored in the adapter. If this keyword
                         is included, the specified address will be used
                         instead of the adapter's actual node address.

        PORT          -  This keyword specifies the I/O base address
                         used by the adapter. This value must match the
                         actual I/O base address setting on the adapter.
                         If this keyword is not specified, the default
                         value will be put into effect.

        INT           -  This keyword specifies the interrupt line used
                         by the adapter. This value must match the actual
                         IRQ setting on the adapter. If this keyword is
                         not specified, the default value will be put
                         into effect.

        FRAME        -  This keyword specifies the supported frame types.
                        Four types are available:

                        ETHERNET_802.3, ETHERNET_802.2,
                        ETHERNET_II and ETHERNET_SNAP.

        AUTOSENSE     - Auto detect the speed and duplex mode.

        100_Half      - User force the media to 100 Mbps and half duplex
                        mode.

        10_Full       - User force the media to 10 Mbps and full duplex
                        mode.

        10_Half       - User force the media to 10 Mbps and half duplex
                        mode.
