==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
for Windows 98 Users
==================================================================
(c) 1998 Copyright D-Link ALL RIGHTS RESERVED

This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen instructions,
for Windows 98 users regarding DFE-650 Fast Ethernet PC Card installation.


Win98 users, please also refer to the following.

     -------------------------------------------------------------------
        File              Description/Installation Notes
     -------------------------------------------------------------------
        README.TXT        Overall installation notes for all users


Follow these steps to install the DFE-650 Fast Ethernet PC Card's driver:

    1. Start your PC, then insert the DFE-650 Fast Ethernet
       PC Card into an available PC Card slot in your PC .

    2. After starting Windows 98, the DFE-650 Fast Ethernet PC Card will
       be detected automatically, then the Add New Hardware Wizard
       window appears.

    3. Insert the DFE-650 Fast Ethernet PC Card Installation diskette
       into floppy disk drive.

    4. Click the Next button in the Update Device Driver Wizard window.
       Win98 will start to search floppy drive A for network driver,
       and Windows displays the message

            "D-Link DFE-650 Fast Ethernet PC Card"

    5. Click Finish button,
       then the Win98 starts to copy the DFE-650 Fast Ethernet PC Card
       driver to the user's hard disk.

    6. Restart your computer.


