InS_StArT
DFE650.COM
1.0
^D-Link DFE-650 Fast Ethernet PC Card,DFE650.COM,IE0
?Please select the options that match your board's IO settings.
!RIE0(PORT)
@300
320
340
360
380
240
260
280
2A0
2C0
2E0
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
