==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For Client 32 for Windows 95 and DOSWIN Users
==================================================================
    (c) 1998 Copyright D-Link ALL RIGHTS RESERVED



This document contains DFE-650 Fast Ethernet PC Card installation
notes, which is not included in the DFE-650 Fast Ethernet PC Card
USER'S GUIDE or onscreen instructions, for Client 32 for Windows 95
and DOSWIN users.


This document contains information on the following topics:

1.0   Overview
2.0   Installation Notes For  Client 32 for Windows 95 users
       2.1   Install DFE-650 Fast Ethernet PC Card for the first time
       2.2   DFE-650 Fast Ethernet PC Card Driver Reinstallation
3.0   Installation Notes For Client 32 for DOSWIN users
       3.1  Windows 3.x Users
       3.2  DOS Users
___________________________________________________________________



1.0 Overview
------------

      To install DFE-650 in the  Client 32 for Windows 95 environment,
      you should have the Windows 95 CD-ROM and the NOVELL Client 32
      CD-ROM nearby.

2.0  Installation Notes for Client 32 for Windows 95 users
----------------------------------------------------------

 2.1   Install DFE-650 Fast Ethernet PC Card for the first time
 --------------------------------------------------------------
        1. Start the Windows 95 system.
           Note:
                Don't insert your DFE-650 Fast Ethernet PC Card into
                a PC Card slot.

        2. If you have installed DFE-650 Fast Ethernet PC Card NDIS3
           driver.
           Do the following steps.
           2.1 Double click on "My Computer" icon under desktop.
           2.2 Double click on "Control Panel" icon under "My Computer"
               window.
           2.3 Double click on "Network" icon under "Control Panel"
               window.
           2.4 Select "D-Link DFE-650 Fast Ethernet PC Card" item and
               click on [ Remove ] button. Click on [ OK ] button after
               the adapter have been removed under "Network" window.
           2.5 Click on [ No ] button under "System Settings Chagne"
               window.
           2.6 Please change the directory to C:\WINDOWS\INF
               2.6.1 Click on [ Start ] button.
               2.6.2 Select "Programs" -> "MS-DOS Prompt" item.
               2.6.3 Type the following command.
                     C:\WINDOWS>cd inf
                     C:\WINDOWS\INF>md temp
                     C:\WINDOWS\INF>copy netdf650.inf temp\*.*
                     C:\WINDOWS\INF>del netdf650.inf
                     C:\WINDOWS\INF>exit

        3. Run the Client 32 for Windows 95 installation program
           using SETUP.EXE and accept the agreement.

           Example:
             Click "Start" -> "Programs" -> "Windows Explorer"
              to find the Client 32 for Windows 95 SETUP.EXE.
              Double click SETUP icon in <PATH>\WIN95 directory.

        4. Check the box of "Upgrade NDIS drivers to ODI automatically,
           if available" and press [ Start> ] button.

        5. Click on [ Cancel ] button under "Select Device" window.

        6. Click on [ Cancel ] button under "Select Device" window.

        7. Click on [ Cancel ] button under "Select Device" window.

        8. Click on [ Yes ] button under "Recommended NetWare Client 32
           Properties" window.

        9. Specify NetWare Preferred server name and First network drive
           under "Novell NetWare Client 32 Properties" windos then click
           on [ Yes ] button.

       10. Click on [ OK ] button under "Installation Aborted" window.

       11. Click on [ OK ] button under "Network" window.

       12. Click on [ No ] button under "System Settings Change" window.

       13. Please insert your DFE-650 Fast Ethernet PC Card into
           a PC Card slot.

       14. Windows 95 system will find the Ethernet PC Card.

       15. Select "Driver from disk provided by hardware manufacturer"
           item then click on [ OK ] button under "New Hardware Found"
           window.

       16. Please insert release driver diskette into the disk drive.

       17. Specify the full path of the driver under "Install From Disk"
           window.

           Example: A:\NETWARE\32BITLAN

       18. Click on [ Yes ] button under "System Settings Change" window
           to reboot your Windows 95 system.


 2.2   DFE-650 Fast Ethernet PC Card Driver Reinstallation
 ---------------------------------------------------------

        1. Assume your Windows 95 and Client 32 for Windows 95 system
           have been installed successfully.

        2. Start the Windows 95 system.
           Note:
                Don't insert your DFE-650 Fast Ethernet PC Card into
                a PC Card slot.
        3. If you have installed DFE-650 Fast Ethernet PC Card NDIS3
           driver.
           Do the following steps.
           3.1 Double click on "My Computer" icon under desktop.
           3.2 Double click on "Control Panel" icon under "My Computer"
               window.
           3.3 Double click on "Network" icon under "Control Panel"
               window.
           3.4 Select "D-Link DFE-650 Fast Ethernet PC Card" item and
               click on [ Remove ] button. Click on [ OK ] button after
               the adapter have been removed under "Network" window.
           3.5 Click on [ No ] button under "System Settings Change"
               window.
           3.6 Please change the directory to C:\WINDOWS\INF
               2.6.1 Click on [ Start ] button.
               2.6.2 Select "Programs" -> "MS-DOS Prompt" item.
               2.6.3 Type the following command.
                     C:\WINDOWS>cd inf
                     C:\WINDOWS\INF>md temp
                     C:\WINDOWS\INF>copy netdf650.inf temp\*.*
                     C:\WINDOWS\INF>del netdf650.inf
                     C:\WINDOWS\INF>exit

        4. Please insert DFE-650 Fast Ethernet PC Card into
           a PC Card slot.

        5. Windows 95 system will find the PC Card.

        6. Select "Driver from disk provided by hardware manufacturer"
           item then click on [ OK ] button under "New Hardware Found"
           window.

        7. Please insert release driver diskette into the disk drive.

        8. Specify the full path of the driver under "Install From Disk"
           window.

           Example: A:\NETWARE\32BITLAN

        9. Click on [ Yes ] button under "System Settings Change" window
           to reboot your Windows 95 system.

    2.3  Keywords supported by DFE650
    ----------------------------------

         Connection Type - This keyword specifies that the duplex mode and
                        line speed on network cards.


 3.0  Installation Notes for Client 32 for DOSWIN users
 --------------------------------------------------------------------
  *******************************************************************
  * Notes: The PC Card should be enabled by Card services.          *
  *        Please run DFCD.EXE before starting Client 32 for DOSWIN.*
  *                                                                 *
  *        Content of CONFIG.SYS                                    *
  *        ---------------------                                    *
  *        Add below two lines to the CONFIG.SYS file               *
  *                                                                 *
  *        DEVICE=C:\DOS\EMM386.EXE NOEMS X=D000-D7FF               *
  *        DEVICE=<PATH\DFCD.EXE /iop=300 /irq=11                   *
  *        ; <PATH> is a directory that includes the DFCD.EXE file. *
  *        ; Please refer to the INST_DOS.TXT file for details.     *
  *******************************************************************


3.1  Windows 3.x Users
----------------------

    1. Start Windows 3.x system
    2. Run the Client 32 for DOSWIN installation program, using SETUP.EXE

        Example: >CD \<PATH>        ; <PATH> is Client 32 for DOSWIN
                 >SETUP.EXE

           or

          Double click SETUP.EXE in Files Manager windows

    3. Press ENTER to accept the agreement.
    4. Specify your target directory.

       Example: C:\NOVELL\CLIENT32  ; If you had chosen the C drive.

    5. Click "Other Boards..."

    6. Please insert release driver diskette into the disk drive.

    7. Specify the full path of the driver, i.e. A:\<PATH>.

       Example: A:\NETWARE\32BITLAN\DFE650.LAN

    8. Select "D-Link DFE-650 Fast Ethernet PC Card Driver".
    9. Specify your configuration for Additional Optional window
       then click "Next>" to continue.
   10. Restart your workstation, click "NetWare Login" to login to the
       NetWare server from NetWare Tools.
   11. Keywords supported by DFE650


       Connection Type - This keyword specifies that the duplex mode and
                        line speed on network cards.

 3.2  DOS Users
 --------------------
        1. Run the Client 32 for DOSWIN installation program, using
           INSTALL.EXE.

           Example: >CD \<PATH>         ; <PATH> is Client 32 for DOSWIN
                    >INSTALL.EXE

        2. Press ENTER or YES to accept the agreement.
        3. Select "NetWare Client 32 for DOS".
        4. Use default value in Customize Support for Windows
           if you Select "NetWare Client 32 for Windows", as well.
        5. Press "F10" to continue.
        6. Select "32-bit LAN drivers" from LAN Driver Type window.
        7. Select "USER SPECIFIED 32 BIT DRIVER".
        8. Please insert release driver diskette into the disk drive.
        9. Specify the full path of the driver, i.e. A:\<PATH>.

           Example: A:\NETWARE\32BITLAN

       10. Select "D-Link DFE-650 Fast Ethernet PC Card Driver" from
           32-Bit Network Board Drivers window.
       11. Specify "Connection Type", "Driver Retries", "Frame Type"
           "Node Address" setting, then press "F10" to save.

           Example: Default value is as below
               Frame Type is Ethernet_802.2
               Slot       is 1

       12. Press "F10" to continue in Installation Configuration Summary
           window, if you accept.
       13. AUTOEXEC.BAT and CONFIG.SYS will be update after installation.
       14. Restart your workstation and load the NetWare networking
           software; it will connect to the Netware server.

       15. Keywords supported by DFE650

           Connection Type - This keyword specifies that the duplex mode and
                        line speed on network cards.

  ******************************************************************
  * Notes: The PC Card should be enabled by Card service.          *
  *       Please run DFCD.EXE before starting Client 32 for DOSWIN.*
  *                                                                *
  *        > DFCD /iop=300 /irq=11                                 *
  ******************************************************************
