==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For SUN PC-NFS V5.0 Users
==================================================================
(c) 1998 Copyright D-Link Corporation  ALL RIGHTS RESERVED



This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen instructions,
for SUN PC-NFS V5.0 users regarding DFE-650 Fast Ethernet PC Card
installation.


This document contains information on the following topics:

1.0 Introduction
2.0 Installation Notes
___________________________________________________________________


1.0 Introduction
----------------

SUN PC-NFS V5.0 users please also refer to the following:

    -------------------------------------------------------------------
     File                  Description/Installation notes
    -------------------------------------------------------------------
     \PKTDRV\README.TXT    For all Packet driver users


 2.0 Installation Notes
---------------------------

        If user prefers to use ODI MLID driver , please refer to
        the \NETWARE\PCNFS.TXT.

        If user prefers to use NDIS driver , please refer to the
        \NDIS\PCNFS.TXT.

        Packet Driver
        ---------------------
        When using PC-NFS independently, select the "OTHER" option from
        the PC-NFS installation screen.  This option works with the
        PACKET driver included in the provided driver diskette.  Copy
        the files listed below into the \NFS directory of your hard disk.
        These files will be used in the installation.

        File             Description
        ------------     -------------------------------------
        PDNFS.SYS        PC-NFS driver program
        DFE650PD.SYS      Packet driver program


        The following lists the contents of the configuration files:

        CONFIG.SYS                             AUTOEXEC.BAT
        ------------------                     ------------------------
        SWITCHES=/F                            SET TZ=EST5EDT
        DEVICE=C:\HIMEM.SYS                    C:\DOS\SMARTDRV.EXE
        DEVICE=C:\EMM386.EXE NOEMS X=D000-D7FF @PROMPT $p$g
        DOS=HIGH,UMB                           PATH=C:\NFS;C:\DOS;
        BUFFERS=10,0                           SET TEMP=C:\DOS
        FILES=40                               SET NFSDRIVE=C
        STACKS=0,0                             SET NFSPATH=C:\NFS
        LASTDRIVE=G                            SET TN_DIR=C:\NFS\TELNET
        SHELL=C:\DOS\COMMAND.COM C:\DOS /P     C:\NFS\PRT *
        DEVICE=C:\NFS\PCNFS.SYS /l40           C:\NFS\NET INIT
        DEVICE=C:\NFS\SOCKDRV.SYS
        DEVICE=C:\NFS\DFE650PD.SYS
        DEVICE=C:\NFS\PDNFS.SYS
