#
# Data file of install program
#
#  char far * far N_List[]
# no. item of N_List[] Company name selection
4
# item of N_List[]
# Maxlen , "string"
#20,"D-Link         "
20,"IBM            "
20,"Microsoft      "
20,"Novell         "
20,"Others         "
#
# ID of N_NosList[] item
#100
101
102
103
104
#  char far * far N_ListSta[]
# no. item of N_ListSta[] Company name selection status line
4
# item of N_List[]
#80,"Press Enter/Tab key to display D-Link network operating systems. "
80,"Press Enter/Tab key to display IBM network operating systems. "
80,"Press Enter/Tab key to display Microsoft network operating systems. "
80,"Press Enter/Tab key to display Novell network operating systems. "
80,"Press Enter/Tab key to display others network operating systems. "
#----------------------------------------------------------------------------
#  char far * far DL_NosList[]
# no. item of DL_NosList[] nos selection
#2
# item of N_NisList[]
#25,"LANsmart                 "
#25,"TCP/IP for DOS           "
# ID of N_NosList[] item
#8
#9
#  char far * far DL_NosSta[]
# no. item of DL_NosSta[] nos selection status line
#2
# item of DL_NosSta[] (MaxLen,string)
#80,"Copy D-Link LANsmart drivers to target path. "
#80,"Copy D-Link TCP/IP for DOS drivers to target path.    "
#---------------------------------------------------------------------------
#  char far * far IBM_NosList[]
# no. item of IBM_NosList[] nos selection
5
# item of NVL_NosList[]
30,"IBM OS/2 LAN Server        "
30,"IBM LAN Service v4.0       "
30,"IBM LAN Support program    "
30,"IBM OS/2 warp Server       "
30,"IBM OS/2 warp Connection   "
# ID of NVL_NosList[] item
11
10
10
11
11
# no. item of IBM_NosSta[] nos selection status line
5
# item of IBM_NosSta[]
80,"Display install procedures of adapter drivers for IBM LAN Server v3.x/v4.x. "
80,"Display install procedures of adapter drivers for IBM LAN Service v4.x. "
80,"Display install procedures of adapter drivers for IBM LAN Support program. "
80,"Display install procedures of adapter drivers for IBM OS/2 warp Server v4.x."
80,"Display install procedures of adapter drivers for IBM OS/2 warp connection. "
#---------------------------------------------------------------------------
#  char far * far MS_NosList[]
# no. item of MS_NosList[] nos selection
6
# item of MS_NosList[]
30,"Microsoft Windows 98          ",
30,"Microsoft Windows 95          ",
30,"Microsoft Windows NT v4.0     ",
30,"Microsoft Windows NT v3.51    ",
#30,"Microsoft Windows NT v3.5     ",
#30,"MS Window for Workgroup v3.11 ",
30,"Microsoft Client for DOS   ",
30,"Microsoft LAN Manager for DOS ",
# ID of MS_NosList[] item
43
29
15
30
#16
#14
40
12
# no. item of MS_NosSta[] nos selection status line
6
# item of MS_NosSta[]
80,"Display install procedures of adapter drivers for MS Windows 98."
80,"Display install procedures of adapter drivers for MS Windows 95."
80,"Display install procedures of adapter drivers for MS Windows NT v4.0."
80,"Display install procedures of adapter drivers for MS Windows NT v3.51."
#80,"Display install procedures of adapter drivers for MS Windows NT v3.5."
#80,"Display install procedures of adapter drivers for MS WFW v3.11"
80,"Display install procedures of adapter drivers for MS Client DOS v3.0."
80,"Display install procedures of adapter drivers for MS LAN Manager for DOS."
#---------------------------------------------------------------------------
#  char far * far NVL_NosList[]
# no. item of NVL_NosList[] nos selection
5
# item of NVL_NosList[]
40,"Novell NetWare Client for DOS  "
40,"Novell NetWare v4.x Server   "
40,"Novell NetWare v3.12 Server  "
#40,"Novell NetWare v3.11 Server  "
40,"Novell NetWare Client 32 for Windows 95"
#40,"Novell NetWare Client 32 for Windows NT "
40,"Novell NetWare Client 32 for DOS/WIN  "
#40,"Novell Lan Workplace         "
#40,"Novell NetWare Client for OS/2  "
# ID of NVL_NosList[] item
21
5
4
#3
26
#41
31
#32
#2
# no. item of NVL_NosSta[] nos selection status line
5
# item of NVL_NosSta[]
80,"Copy Novell NetWare DOS Client drivers to target path.   "
80,"Display install procedures of adapter drivers for NetWare Server v4.x."
80,"Display install procedures of adapter drivers for NetWare Server v3.12."
#80,"Copy Novell NetWare v3.11 Server drivers to target path. "
80,"Display install procedures of adapter drivers for NetWare Client 32 Win 95."
#80,"Display install procedures of adapter drivers for NetWare Client 32 Win NT."
80,"Display install procedures of adapter drivers for NetWare Client 32 DOS/WIN"
#80,"Copy Novell Lan Workplace drivers to target path.        "
#80,"Copy Novell NetWare OS/2 Client drivers to target path.  "
#
#---------------------------------------------------------------------------
#  char far * far OTHERS_NosList[]
# no. item of OTHERS_NosList[] nos selection
6
# item of OTHERS_NosList[]
#30,"SCO Unix drivers          "
#30,"AT&T Unix drivers         "
30,"Winsock for Internet      "
30,"PC/TCP                    "
30,"DEC Pathworks             "
30,"PC-NFS v5.0               "
30,"Banyan VINES              "
30,"NCSA                      "
#30,"Lantastic                 "
# ID of OTHERS_NosList[] item
#23
#22
33
34
36
27
37
28
#17
# no. item of OTHERS_NosSta[] nos selection status line
6
# items of OTHERS_NosSta[]
#80,"Display install procedures of adapter driver for SCO Unix.  "
#80,"Display install procedures of adapter driver for AT&T Unix.  "
80,"Copy Winsock for Internet drivers to target path.   "
80,"Copy PC/TCP drivers to target path.                 "
80,"Copy DEC Pathworks drivers to target path.          "
80,"Copy PC-NFS v5.0 drivers to target path.            "
80,"Copy Banyan VINES drivers to target path.          "
80,"Copy NCSA drivers to target path.          "
#80,"Display install procedures of adapter driver for Lantastic.  "
# *************************NORMAL MESSAGE*****************************
# --------Welcome MESSAGE-----------
4
# items of Welcome msg
72," Welcome to D-Link Ethernet PC Card installation program, The program "
72," helps you setup your adapter. "
72," "
72," To continue, press Enter key. To exit, press Esc."
#---main menu list------------
4
32,"View/Print General Information"
60,"Quick Install 16-bit Driver for DOS NetWare Client"
48,"View/Print Installation Instructions"
40,"Install Diagnostic program"
#---main menu list status-----------
4
80,"View/print Release notes"
80,"Automatic installation of 16-bit software for DOS-based Netware client"
80,"Select/View/Print applicable driver installation instructions."
80,"Install diagnostic program. "
#---Print success---
2
50," Print completed .  "
50," <Enter> to continue."
#---Exit comfirm ---
1
66,"  Do you really want to exit Installation Director? (N or Y)  "
#---Q Install bye message-------
12
64," Installation completed ! "
64," "
64," Newly  installed  modules will be  loaded and  ready to use  "
64," immediately after restarting the notebook PC."
64," "
64," 1.AUTOEXEC.BAT file have been modified,and prior content has been "
64,"   saved as AUTOEXEC.OLD."
64," 2.NET.CFG file has been modified, and prior content has been saved "
64,"   as NET.OLD . "
64," 3.Please remove floppy disks in preparation for restart."
64," "
64," Restart the notebook PC now?(Y/N) "
#---Query Run Hardware config Msg------
5
68," "
68," Files related to Diagnostic are installed completed."
66," "
66," Do you want to run the Diagnostic program ? (Y/N) "
66," "
9
74," If any network driver is already loaded, then proceeding with this "
74," installation may cause a system halt. You might choose,  as a "
74," precaution, to unload any currently loaded network driver. Or You"
74," might choose simply to proceed. Then, in the event of a halt, restart"
74," the computer and unload the conflicting network driver at that time."
74," Then re-run Installation Director. See the Troubleshooting section of"
74," the User's Guide for assistance on unloading a conflicting driver."
74," "
74," Checking adapter , please wait..... "
#---Change diskette-
3
74," Please insert Disk1 to drive A: "
74," "
74," Then press Enter to continue , Esc to previous menu . "
#---Change diskette-
3
74," Please insert Disk2 to drive A: "
74," "
74," Then press Enter to continue , Esc to previous menu . "
#---Insert Card-
9
74," If any network driver is already loaded, then proceeding with this "
74," installation may cause a system halt. You might choose,  as a "
74," precaution, to unload any currently loaded network driver. Or You"
74," might choose simply to proceed. Then, in the event of a halt, restart"
74," the computer and unload the conflicting network driver at that time."
74," Then re-run Installation Director. See the Troubleshooting section of"
74," the User's Guide for assistance on unloading a conflicting driver."
74," "
74,"          <Enter> to continue          <Esc> to exit "
#---HW configuration copy complete and warning msg -------
7
74," Files related to Diagnostic are installed completed."
74," "
74." The Diagnostic program must execute in a DOS System ,  "
74," Note that be sure don't execute the diagnostic program "
74," in a none DOS system ( Windows 95 , Windows NT ,OS/2 ) "
74," "
74,"         Press Esc to previous menu. "
6
74," Version not match ! "
74," the DLINK.CLB file in the systemsoft directory  is too old,"
74," The install program will update the new DLINK.CLB to your"
74," system ,  After copying completed  we will reboot your system."
74," "
74," Do you want to starting file copy (Y/N)? "
6
74," The DLINK.CLB file updated completed ! "
74," "
74," Please reboot the system ,  then execute the installation "
74," program . "
74," "
74,"                   Press Esc to quit  "
#---Insert Card and Check EMM386 -
13
74," ERROR: DFE-650 PC Card not detected by system.
74," "
74," 1.Exit from Installation Director, then repeat Step 1 of the Hardware"
74,"   Installation procedure given at the  beginning of Chapter 2 of the "
74,"   User's Guide. Then re-run the Installation Director."
74," "
74," 2.After you have ascertained that your DFE-650 PC Card is properly"
74,"   installed in its slot,    and have re-run  Installation Director"
74,"   according to the above Paragraph1,   then in the event that this"
74,"   error re-appears,  see the Troubleshooting section of the User's"
74,"   Guide."
74," "
74,"      <Enter> to continue        <Esc> to return to previous menu "
#---Readme files menu select-----------
3
35,"Release Notes for All Environments"
35,"Release Notes for DOS Platforms"
35,"Release Notes for OS/2 Platforms"
#---Readme files menu list status-----------
3
80,"View/print release notes applicable to all environments"
80,"View/print release notes applicable to DOS platforms"
80,"View/print release notes applicable to OS/2 platforms"
# **************************HELP MESSAGE***************************
# no. item of instselecthlp1
5
# items of instselecthlp1
74, " Quick Install will copy the 16-bit ODI driver for NetWare Client,"
74, " and related files to the target directory,  then complete the "
74, " installation by copying CONFIG.SYS to CONFIG.OLD, then modifying"
74, " CONFIG.SYS,  and copying  AUTOEXEC.BAT to AUTOEXEC.OLD,  then "
74, " modifying AUTOEXEC.BAT. "
# no. item of instselecthlp2
5
# items of instselecthlp2
74, " Installation Director will lead you to the software installation "
74, " instructions appropriate to your platform OS and network environment."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and the required files"
74, " over from the DFE-650 Software Diskette."
# no. item of instselecthlp3
2
# items of instselecthlp3
74, " Installation Director will Install the diagnostic/troubleshooting"
74, " Program. "
4
# items of DLinkhlp
74, " Choose this function to install D-Link LANsmart and TCP/IP drivers. "
74, " The program copies all device drivers into a user-definable directory "
74, " path. Please follow the instructions from each readme file content at "
74, " the end of the file copying process to complete the installation.  "
# items of IBMhlp
3
74, " Choose this function to install drivers for the NOSs developed by "
74, " IBM . Please follow the instructions from each readme file "
74, " to complete the installation.  "
# items of MShlp
3
74, " Choose this function to install drivers for the NOSs developed by "
74, " Microsoft. Please follow the instructions from each readme file "
74, " to complete the installation.  "
# items of Novelllp
4
74, " Choose this function to install drivers for the NOSs developed by Novell."
74, " The program copies all device drivers into a user-definable directory "
74, " path. Please follow the instructions from each readme file content at "
74, " the end of the file copying process to complete the installation.  "
# items of Othershlp
4
74, " Choose this function to install drivers for the other popular NOSs. "
74, " The program copies all device drivers into a user-definable directory "
74, " path. Please follow the instructions from each readme file content at "
74, " the end of the file copying process to complete the installation.  "
# items of Lansmarthlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                   "
# items of Dlktcphlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                    "
# items of Lansrvhlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of Win95hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NT40hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NT351hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NT35hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of LanMgrhlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of DOSclienthlp
4
74, " Choose this function to install NetWare ODI client driver for DOS.  "
74, " The program copy the device drivers to a user-specified directory,  "
74, " Please  follow  the  instructions  in  the  README  file  upon  "
74, " completion  of the file copy process . "
# items of NWSrv4xhlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NWSrv312hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NWclient32hlp DOS/WIN
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of LanWkPlacehlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of OS2Clienthlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of Scounixhlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of Winsockhlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of PCTCPhlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of Pathworkhlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of Pcnfshlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of Vineshlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of FrmTypehlp
4
74, "        frame type         Help                                      "
74, "                                                                     "
74, "                                                                     "
74, "                                                                     "
# items of TargetPathhlp
4
74, " This field offers a default path and target directory name. Accept"
74, " the default, or type in a different path and a target directory "
74, " name. If the named target directory does not exist, then it will "
74, " be created."
# items of NWSrvNamehlp
2
74, " If you wish to control selection of your preferred Netware server,"
74, " then type in the name of Server. "
# items of NWUserNamehlp
3
74, " Type in your Netware login name. If this field is left blank, then  "
74, " the startup program(AUTOEXEC.BAT) will prompt you for login name and"
74, " wait for your response.                                             "
# items of MdyAutohlp
5
74, " If answer Yes, your existing AUTOEXEC.BAT will be renamed to     "
74, " AUTOEXEC.OLD, and a new AUTOEXEC.BAT will be created.            "
74, " If answer No, an AUTOEXEC.NEW file will be created in the root   "
74, " directory of your boot disk, and you may modify AUTOEXEC.BAT any "
74, " time to invoke the network adapter drivers.                      "
# items of MdyConfhlp
4
74, " If answer Yes, your existing CONFIG.SYS will be renamed to     "
74, " CONFIG.OLD, and a new CONFIG.SYS will be created.              "
74, " If answer No, a CONFIG.NEW file will be created in the root    "
74, " directory of your boot disk.                                   "
# items of NWclient3295hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of WFW311hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NWclient32NThlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NWSrv311hlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of MSClientDOS
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of IBMLAnSupporthlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NCSAhlp
4
74, " Choose this function to copy the device driver files to a user-   "
74, " specified directory.    Please follow the instructions in the     "
74, " README file upon completion of the file copied process.     "
74, "                                                                     "
# items of Lantastichlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve1hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve2hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve3hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve4hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve5hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve6hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve7hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
# items of NosReserve8hlp
6
74, " Installation Director will display software installation instructions"
74, " appropriate to your platform OS and the highlighted network type."
74, " For certain DOS-platform cases, Installation Director will first "
74, " request that you designate a target directory, and will copy the "
74, " required files over from the DFE-650 Software Diskette.  "
74, " "
## ***********************ERROR MESSAGE****************************
3
50,"Printer write error !  "
50,"Please make sure the printer is ready"
50,"then print again."
4
50," Invalid Target Path ! "
50," Please keyin the correct full path "
50," For example:                       "
50," C:\PATH , or B:\PATH , or B:\      "
4
50," Target drive not exist ! "
50," Please input an exist drive in "
50," target path field .  "
50,"
4
50," Target drive not ready ! "
50," Please check the target drive . "
50,"                                "
50," Press Esc to exit , others to try again "
4
50," Write protected error ! "
50," Please check the diskette in  "
50," the target drive.           "
50," Press Esc to exit , others to try again "
6
60," "
70," 'Quick install for NetWare Client'  will  only run  with "
70," PC Card. Please make sure you have a exact PC Card "
70," on your system before you run install and choose "
70," 'Quick install for NetWare Client' next time. "
60," "
6
65," The PC Card can not be enabled !   "
65," Because we do not support the PC Card chipset in the machine. "
65," Please contact the vendor of PC Card for technical "
65," support. "
65," Press Esc to exit. "
65," "
6
60," "
60," The PC Card can not be enabled ! "
60," Check the EMM386 setting in the CONFIG.SYS file "
60," Exp : EMM386 X=D000-D7FF    "
60," "
60," Press Esc to exit . "
14
74," "
74," The  PC Card can not be  properly detected.  There might be some "
74," problems in your PC Card environment.  Please  re-check your PC Card "
74," environment  including  Socket Services,  Card Services  installation."
74," And make sure loading EMM386 by correct parameter in config.sys file: "
74,"  <For Phoenix PCM Plus>  "
74,"        in  CONFIG.SYS  file           "
74,"                 :                                "
74,"      DEVICE=C:\\path\\EMM386 X=C800-D7FF  ";
74," "
74,"Please correct any mistake, reboot your PC and run Install program again."
74,"If you see this message more than twice ,please contact the PC Card "
74,"vendor for technical support. "
74,"                         Press Esc to exit . "
14
74," "
74," The  PC Card cannot be  properly detected.  There might be some"
74," problems in your PC Card environment.  Please re-check your PC Card "
74," environment  including  Socket Services,  Card Services  installation."
74," And make sure loading EMM386 by correct parameter in config.sys file: "
74,"  <For System Soft>  "
74,"        in  CONFIG.SYS  file                         "
74,"                 :                                "
74,"      DEVICE=C:\\path\\EMM386 X=D000-D7FF  "
74," "
74,"Please correct any mistake, reboot your PC and run Install program again."
74,"If you see this message more than twice ,please contact the PC Card"
74,"vendor for technical support. "
74,"                        Press Esc to exit . "
14
74," "
74," The  PC Card can not be properly detected.  There might be some"
74," problems in your PC Card environment.  Please  re-check your PC Card "
74," environment  including  Socket Services,  Card Services  installation."
74," And make sure loading EMM386 by correct parameter in config.sys file: "
74,"  <For AMI>  "
74,"        in  CONFIG.SYS  file                         "
74,"                 :                                "
74,"      DEVICE=C:\\path\\EMM386 X=D000-DBFF  "
74," "
74,"Please correct any mistake, reboot your PC and run Install program again."
74,"If you see this message more than twice ,please contact the PC Card"
74,"vendor for technical support. "
74,"                        Press Esc to exit . "
14
74," "
74," The  PC Card can not be  properly detected.  There might be some"
74," problems in your PC Card environment.  Please  re-check your PC Card "
74," environment  including  Socket Services,  Card Services  installation."
74," And make sure loading EMM386 by correct parameter in config.sys file: "
74,"  <For Award CardWare>  "
74,"        in  CONFIG.SYS  file                         "
74,"                 :                                "
74,"      DEVICE=C:\\path\\EMM386 X=CF00-D7FF  "
74," "
74,"Please correct any mistake, reboot your PC and run Install program again."
74,"If you see this message more than twice ,please contact the PC Card "
74,"vendor for technical support. "
74,"                       Press Esc to exit . "
10
74," "
74," Your PC Card environment is not entire,  To assist in troubleshooting, "
74," please take note of the notebook vendor information including "
74," manufacturer and model. Make a copy of the  AUTOEXEC.BAT and  CONFIG.SYS"
74," files and contact your local authorized dealer, distributor or branch "
74," office for technical support."
74," "
74," "
74," "
74,"                      Press Esc to exit . "
# *********************OTHER MESSAGE*******************************
# no. of message
57
# messages
6,"Esc"
6,"Exit"
6,"Enter"
8,"Continue"
2,""
12,"Select Item"
2, "F3"
2, "F4"
2, "F5"
2, "F2"
2, "F1"
6, "Help"
10,"Prev menu"
6,"Readme"
4,"Quit"
8, "Scroll"
6, "Print"
16,"Select readmes"
22," Select machine type "
18," Main menu "
50," The network operating system configuration is : "
30,"Network System or Client ->"
14,"Driver Type :"
12,"Frame Type :"
46,"Files to be copied to target directory ->"
20,"Target Directory : "
22,"Modify Autoexec.bat ? "
20,"Modify Config.sys ? "
80,"Press Enter to select company name of your network operating system."
80,"Press Enter to select frame type of your network operating system."
80,"Typing in a home directory name to hold the PC Card driver and related files"
74,"Allow install program to modify CONFIG.SYS file;   Toggle by Space key. "
74,"Allow install program to modify AUTOEXEC.BAT file;  Toggle by Space key. "
18,"Copying files : "
40,"Software copies completed !"
54,"Press any key to view/print installation notes..."
76," D-Link DFE-650 Ethernet PC Card Installation Director         V3.1 "
40,"Name of your Preferred NetWare Server : "
36,"Your NetWare login name : "
80,"Type name of your preferred NetWare file server. "
80,"Type your Novell NetWare login name."
60,"Install Diagnostic programs : "
50,"<Enter> to proceed with installation "
12,"Install : "
12,"Error"
14,"Selected ->"
60," Diagnostic programs "
28,"Card and Socket Service ->"
26,"Based I/O address ->"
40,"IRQ(interrupt) number for DFE-650 ->"
40," Please input the path of CardSoft : "
12,"None"
40," Please input the path of Disk1 : "
40," Please input the path of Disk2 : "
40," General Information "
40," Highlight LAN Vendor or Type "
40," Highlight Specific NOS or Client "
