==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
for Windows 95 Users
==================================================================
(c) 1998 Copyright D-Link ALL RIGHTS RESERVED

This document contains installation notes, which is not included in the
DFE-650 Fast Ethernet PC Card USER'S GUIDE or onscreen instructions,
for Windows 95 users regarding DFE-650 Fast Ethernet PC Card installation.


Win95 users, please also refer to the following.

     -------------------------------------------------------------------
        File              Description/Installation Notes
     -------------------------------------------------------------------
        README.TXT        Overall installation notes for all users



This document contains information on the following topics:

1.0 Installation Notes For Win95 OSR2 Users
2.0 Installation Notes For Other Win95 Users
___________________________________________________________________




1.0 Installation Notes For Win95 OSR2 Users
___________________________________________


    Follow the steps to install the DFE-650 Fast Ethernet PC Card's driver:

    1. Start your PC, then insert the DFE-650 Fast Ethernet
       PC Card into an available PC Card slot in your PC .

    2. After starting Windows 95, the DFE-650 Fast Ethernet PC Card will
       be detected automatically, then the Update Device Driver Wizard
       window appears.

    3. Insert the DFE-650 Fast Ethernet PC Card Installation diskette
       into floppy disk drive.

    4. Click the Next button in the Update Device Driver Wizard window.
       Win95 will start to search floppy drive A for network driver,
       and Windows displays the message

            "D-Link DFE-650 Fast Ethernet PC Card"

    5. Click Finish button,
       then the Win95 starts to copy the DFE-650 Fast Ethernet PC Card
       driver to the user's hard disk.

    6. Restart your computer.



2.0 Installation Notes For Other Win95 Users
____________________________________________

    Follow the steps to install the DFE-650 Fast Ethernet PC Card's driver:
    1. Start your PC, then insert the DFE-650 Fast Ethernet
       PC Card into an available PC Card slot in your PC .

    2. After starting Windows 95, the DFE-650 Fast Ethernet  PC Card will
       be detected automatically and a driver will be required.
       Please select "Have disk from Manufacture".

    3. Insert the DFE-650 Fast Ethernet installation diskette into floppy
       disk drive.

    4. Type A:\ and click OK button to install DFE-650 Fast Ethernet PC
       Card driver.

    5. Then follow the onscreen installations to complete Windows 95
       installation process, and restart your computer.

