==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For IBM Warp Server, Lan Server and Communication Manager 1.x users
==================================================================
    (c) 1998 Copyright D-Link Corporation ALL RIGHTS RESERVED

This document contains DFE-650 Fast Ethernet PC Card installation notes,
which is not included in the DFE-650 Fast Ethernet PC Card USER'S GUIDE
or onscreen instructions, for IBM Warp Server, Lan Server and
Communication Manager 1.x users.


This document contains information on the following topics:

1.0   Overview
2.0   Installation Notes
        2.1   Installation notes for IBM Warp Server/Warp Connect Users
        2.2   Installation notes for IBM LAN SERVER 4.0 users
        2.3   Installation notes for IBM LAN SERVER 3.0 users
        2.4   Installation notes for IBM Communication Manager users
___________________________________________________________________



1.0 Overview
------------

For IBM Warp Server, Lan Server and Communication Manager 1.x users,
please also refer to the following:

-------------------------------------------------------------------
File                Description/Installation Notes
-------------------------------------------------------------------

\NDIS2\README.TXT   Overall installation notes for all NDIS users


2.0   Installation Notes
-------------------------
     The following describes how to install Lan Server and Communication
     Manager.

   2.1 Installation notes for IBM Warp Server/Warp Connect users
   -------------------------------------------------------------
        1. In the OS/2 Desktop group, double-click on the "LAN Services
           and Protocol Services" icon.

        2. Double-Click the "Adapters and Protocol Services" icon to enter
           the MPTS configuration process.

        3. Click on the <OK> Button.

        4. Click on the <Configure> button.

        5. Select the "LAN adapters and protocols" option.

        6. Click on the <Configure> button.

        7. Select the "Other adapters ..." option.

        8. Insert the driver diskette into Drive A or B and type the
           driver path:

            A:\<PATH>       Where PATH is the driver directory.
                            Ex: \NDIS2\OS2.V3

        9. Click on the <OK> button.

        10. Select "D-Link DFE-650 Fast Ethernet PC Card", and then click
            on the <Add> button.

        11. Select "IBM OS/2 NETBIOS", and then click on the <Add> button.

        12. Select "IBM IEEE 802.2", and then click on the <Add> button.

        13. Click OK.

        14. Click Close.

        15. Click Exit.

        16. Click Exit.

        17. Restart your system.

2.2 Installation notes for IBM LAN SERVER 4.0 users
---------------------------------------------------

        1. In the OS/2 Desktop group, double-click on the LAN Server MPTS
           icon.

        2. Click on the <Configure> button.

        3. Select the "LAN adapters and protocols" option.

        4. Click on the <Configure> button.

        5. Select the "Other adapters ..." option.

        6. Insert the driver diskette in Drive A or B and type the
           driver path:

            A:\<PATH>       Where PATH is the driver directory.
                            Ex: \NDIS2\OS2.V3

        7. Click on the <OK> button.

        8. Select "D-Link DFE-650 Fast Ethernet PC Card", and then click
           on the <Add> button.

        9. Select "IBM OS/2 NETBIOS", and then click on the <Add> button.

        10. Select "IBM IEEE 802.2", and then click on the <Add> button.

        11. Click OK.

        12. Click Close.

        13. Click Exit.

        14. Reboot your system.


2.3 Installation note for IBM LAN SERVER 3.0 users
--------------------------------------------------

        1. Install IBM OS/2 into your system, if not yet installed.

        2. Insert the NTS/2 Adapter & Protocol Support Disk in Drive A.

        3. Execute the LAPs program.

        4. Select "Install", and then specify the target drive.

        5. Select "Install" again and insert the driver diskette in
           Drive A.

        6. Select "Configure".

        7. Select "D-Link DFE-650 Fast Ethernet PC Card",
           and then click on the Add button.

        8. Select "IBM OS/2 NETBIOS", and then click on the Add button.

        9. Select "IEEE 802.2", and then click on the Add button.

        10. Click OK.

        11. Click Exit.

        12. Click Continue.

        13. Reboot your system.

        14. Your CONFIG.SYS and PROTOCOL.INI files should reflect your
            card setup:

            *** Example DEVICE command in the CONFIG.SYS file ***
            -----------------------------------------------------
               :
          Device=C:\IBMCOM\MACS\DFE650.OS2
               :
               :


             *** Example \IBMCOM\PROTOCOL.INI file ***
            -------------------------------------------
           (I) For OS/2 V3.0
                      :
                [DFE650IBM_NIF]
                Drivername = DFE650$


        15. Install the LAN Server or Requester program.  For information,
            please refer to your IBM LAN Server"Planning and Installation"
            manual.


2.4 Installation note for IBM Communication Manager users
---------------------------------------------------------

        1. Install IBM Communication Manager

        2. Copy the DFE650.OS2 and DFE650IB.NIF
           in the driver diskette to the C:\IBMCOM\MACS directory

        3. Select the DFE-650 adapter

        4. Choose the appropriate protocols

        5. Check that the CONFIG.SYS file includes the following line:

           DEVICE = C:\IBMCOM\MACS\DFE650.OS2 (FOR OS/2 V3.0)

        6. Restart your computer
