[D-Link]
Type = NDIS
Title = "D-Link DFE-650 Fast Ethernet PC Card"
Version = 1.0
Drivername = DFE650$
Xports = NETBEUI LANDD

[FILE]
Name = DFE650.DOS
Path = @lanroot\DRIVERS\ETHERNET\DFE650

; Parameter start
[IOADDRESS]
tag = IOADDRESS
display = "I/O Base Address"
type = Hexadecimal
default = 0300
set = 0240,0280,0300,0320,0340,0360
scope = Local
Optional = No
Editable = Yes
Virtual = No
Help = "This parameter specifies the I/O base address for the card.
The valid addresses are 240h, 280h, 300h, 320h, 340h, and 360h."

[INTERRUPT]
tag = INTERRUPT
display = "Interrupt [IRQ]"
Type = Decimal
Default = 3
Set = 3,4,5,9,10,11,12,15
Scope = Local
Optional = No
Editable = Yes
Virtual = No
Help = "This parameter speficies the interrupt line [IRQ] that the adapter
 uses. The valid interrupt lines are IRQ3, IRQ4, IRQ5, IRQ9, IRQ10, IRQ11,
 IRQ12, and IRQ15."

[netaddress]
tag = NETADDRESS
display = "Network adapter address"
type = Hexstring
Strlength = 12
optional = YES
editable = YES
help = "This parameter overrides the network address of the network adapter
 card.  The value of this parameter is a hexadecimal string of 12 gigits, as
 in 020001020304.  The address must be unique among all other network adapter
 addresses on the network."

[CONNECTION]
tag = CONNECTION
display = "Connection Type"
type = string
Strlength = 12
Set = AUTOSENSE, MB100_Half, MB10_Full, MB10_Half
default = AUTOSENSE
optional = YES
editable = YES
help = "This parameter specifies the connection type for the card.
 The valid connection type are AUTOSENSE, MB100_Half, MB10_Full,
 and MB10_Half. "


