==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For NetWare Server 3.12 Driver Users
==================================================================
    (c) 1998 Copyright D-Link Corporation ALL RIGHTS RESERVED



This document contains DFE-650 Fast Ethernet PC Card installation notes,
which is not included in the DFE-650 Fast Ethernet PC Card USER'S GUIDE
or onscreen instructions, for NetWare Server 3.12 Driver users.


This document contains information on the following topics:

1.0   Overview
2.0   Installation notes for NetWare Server 3.12 Driver users
___________________________________________________________________



1.0 Overview
------------

Please also refer to the INST_DOS.TXT file on the DFE-650 Installation
disk.


2.0   Installation Note for NetWare Server 3.12 Driver users
------------------------------------------------------------

  ******************************************************************
  * Notes: The PC Card should be enabled by Card service.          *
  *        Please run DFCD.EXE before starting the server.         *
  *                                                                *
  *        Content of CONFIG.SYS                                   *
  *        ---------------------                                   *
  *        Add below item to the  CONFIG.SYS                       *
  *                                                                *
  *        DEVICE=<PATH>\DFCD.EXE /iop=300 /irq=11                 *
  *        ; <PATH> is a directory include DFCD.EXE file.          *
  *        ; Please refer to the INST_DOS.TXT for details.         *
  ******************************************************************

    Modifying an existing NetWare 3.12 Server
    -----------------------------------------

        1. Make a sub-directory NLMS.OLD under <SRVPATH> directory which
           will include SERVER.EXE file.

           Example:
              <SRVPATH> = SRV312.
              >MD \SRV312\NLMs.OLD

        2. Save NBI31X.NLM, MSM31X.NLM and ETHERTSM.NLM to NLMS.OLD
           the sub-directory.

        3. Please insert release driver diskette into disk drive.

        4. Copy all provided NLM and LAN files into your DOS directory
           which will include the SERVER.EXE file.

           >COPY <PATH>\*.NLM   C:\<SRVPATH>
           >COPY <PATH>\*.LAN   C:\<SRVPATH>

           Example: >COPY A:\NETWARE\32BITLAN\*.NLM C:\SRV312
                    >COPY A:\NETWARE\32BITLAN\*.LAN C:\SRV312

           <PATH> here is the directory where support NLMs and
           DFE650.LAN reside.

        5. Start the NetWare Server.

          > CD \SRV312
          > SERVER

        6. From the Novell Server side, execute "LOAD INSTALL". By typing
           :LOAD INSTALL
           Select <System Option>
           Select <Edit Autoexec.NCF file>

        7. Add the item below into the server's AUTOEXEC.NCF file.

        LOAD C:\SRV312\NBI31X.NLM
        LOAD C:\SRV312\MSM31X.NLM
        LOAD C:\SRV312\ETHERTSM.NLM

        LOAD C:\SRV312\DFE650 SLOT=1 FRAME=Ethernet_802.3
             NAME=DFE650_1_E83
        BIND IPX DFE650_1_E83 NET=xxxx

        LOAD C:\SRV312\DFE650 SLOT=1 FRAME=Ethernet_802.2
             NAME=DFE650_1_E82
        BIND IPX DFE650_1_E82 NET=xxxx

        LOAD C:\SRV312\DFE650 SLOT=1 FRAME=Ethernet_II
             NAME=DFE650_1_EII
        BIND IPX DFE650_1_EII NET=xxxx

        LOAD C:\SRV312\DFE650 SLOT=1 FRAME=Ethernet_SNAP
             NAME=DFE650_1_ESP
        BIND IPX DFE650_1_ESP NET=xxxx

        8. Restart the server.

  ******************************************************************
  * Notes: The PC Card should be enabled by Card service.          *
  *        Please run DFCD.EXE before start server.                *
  *                                                                *
  *        > DFCD /iop=300 /irq=11                                 *
  ******************************************************************

    3.0  Keywords supported by DFE650
    ----------------------------------

      TP              - This keyword specifies that the UTP port on the
                        adapter.

      TP_FULL_DUPLEX  - This keyword selects twisted pair connection to
                        work in full duplex mode.

      LINE_SPEED      - This keyword selects line speed between 10Mbps and
                        100Mbps on network cards.

                        Allowed values are: 10,100

