;****************************************************************************************
;
; DRT2860.inf
;
;   This installation script supports Windows 2000 & XP for the
;   D-Link DWA series USB Wireless LAN Card.
;
;   Copyright (C) 2002-2012 D-Link Corporation. All Rights Reserved.
;   
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %D-Link%
Compatible      = 1
DriverVer       = 08/24/2012, 5.00.03.0000
CatalogFile     = Drt2860.cat

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%D-Link%        = D-Link, NTamd64
                       
[D-Link.NTamd64]               
; DisplayName                  Section                 DeviceID
; -----------                  -------                 --------
%D-Link_3C04.DeviceDesc%       = RT3900P_C2.ndi,       PCI\VEN_1814&DEV_3060&SUBSYS_3C041186
%D-Link_3C05.DeviceDesc%       = RT3900P_C2.ndi,       PCI\VEN_1814&DEV_5360&SUBSYS_3C051186
%D-Link_3C06.DeviceDesc%       = RT3900E3.ndi,         PCI\VEN_1814&DEV_5392&SUBSYS_3C061186

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RT3900E3.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg, SingleBand.reg, PowerContrl_F2.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RT3900P_C2.ndi.NT]
AddReg                  = Common.reg, RT80x86.ndi.NT.reg, SingleBand.reg, AdhocN.reg, Customer2.reg, CoInstOpt_DLink.reg, FastRoaming.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections

[RT3900E3.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog

[RT3900P_C2.ndi.NT.Services]
AddService              = RT80x86, 2, Generic.Service, common.EventLog 

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************

[RT3900E3.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RT3900P_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg 

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
;HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
;HKR, NDI\params\Radio,            type,            0, "enum"
;HKR, NDI\params\Radio,            default,         0, "0"
;HKR, NDI\params\Radio\enum,       1,               0, %Disable%
;HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x0b034040"
HKR, Default,                     BACapability,      0x10001, "0x0b034040"

;
; Wifi Direct settings
;
HKR, ,                            WifiDirectControl,    0x10001, "0x00308078"
HKR, Default,                     WifiDirectControl,    0x10001, "0x00308078"

;
; Enable P2P Video Boost within P2P Group
;
HKR, ,                            P2PVideoBoost,      0, "0"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2BA15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2BA15"

;
; Rssi Delta
;
HKR, ,                            RssiDelta,      0, "6"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,              0, "1"

;
; Enable TGnWifiTest Mode
;
HKR, ,                            TGnWifiTest,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
;HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
;HKR, NDI\params\IEEE80211H,       type,            0, "enum"
;HKR, NDI\params\IEEE80211H,       default,         0, "0"
;HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
;HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,       ParamDesc,       0, %WMMCapable%
HKR, NDI\params\WMMCapable,       type,            0, "enum"
HKR, NDI\params\WMMCapable,       default,         0, "1"
HKR, NDI\params\WMMCapable\enum,  0,               0, %Disable%
HKR, NDI\params\WMMCapable\enum,  1,               0, %Enable%

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, %APSDCapable%
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "1"
HKR, NDI\params\APSDCapable\enum,       0,         0, %Disable%
HKR, NDI\params\APSDCapable\enum,       1,         0, %Enable%

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, %APSDAC_BE%
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "1"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_BE\enum,         1,         0, %Enable%

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, %APSDAC_BK%
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "1"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_BK\enum,         1,         0, %Enable%

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, %APSDAC_VI%
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "1"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_VI\enum,         1,         0, %Enable%

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, %APSDAC_VO%
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "1"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_VO\enum,         1,         0, %Enable%

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "1"
HKR, NDI\params\SmartScan,              ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan,              type,      0, "enum"
HKR, NDI\params\SmartScan,              default,   0, "0"
HKR, NDI\params\SmartScan\enum,         0,         0, %Disable%
HKR, NDI\params\SmartScan\enum,         1,         0, %Enable%

;
; RDG
;
HKR, ,                            RDG,             0, "1"

;
; AllowBW40InBGBand
;
HKR, ,                            AllowBW40InBGBand,      0, "1"

;
; WSC Version2 
HKR, ,                            WSCVersion2,     0x00010001, 0x00000020

;
; WSC 2.0 Testbed for some test items. 
HKR, ,                            WSC20Testbed,     0x00010001, 0x0000000C

;
; AdhocN40MHzAllowed
;
HKR, ,                            AdhocN40MHzAllowed,      0, "0"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, %PSPXlink%
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, %Disable%
HKR, NDI\params\PSPXlink\enum,    1,               0, %Enable%

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Initialize Delay
;
HKR, ,                            InitDelay,     0x00010001, 0x00080000

;
; Power Saving Control
;
HKR, ,                            PSControl,       0x00010001, 0x00000000

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,      0, "1"

;
; Link Speed Status
;
HKR, ,                            LinkSpeedStatus, 0, "0"

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
;HKR, Default,                     NetworkAddress,  0, ""
;HKR, NDI\params\NetworkAddress,   ParamDesc,       0, %LocalNetworkAddress%
;HKR, NDI\params\NetworkAddress,   type,            0, "edit"
;HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
;HKR, NDI\params\NetworkAddress,   default,         0, ""
;HKR, NDI\params\Networkaddress,   optional,        0,  "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, %PSMode%
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, %CAM%
HKR, NDI\params\PSMode\enum,      1,               0, %MAXPSP%

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;
; Reposit Bssid List
;
HKR, ,                BssidRepositTime,       0, "90"


;*******************************************************************************************
; Seperate Setting
[IEEE80211H.reg]
HKR, ,                IEEE80211H,      0, "1"

[CarrierDetect.reg]
HKR, ,                CarrierDetect,   0, "1"

[SmartScan.reg]                   
HKR, ,                SmartScan,       0, "1"

[PowerContrl.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x000000d7

[PowerContrl_C1.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x00000057

[PowerContrl_C2.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x000000d7

[PowerContrlLED.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x00000097

[PowerContrlScan.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x00000017

[PowerContrl_F2.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x000000df

[DisablePowerContrl.reg]
HKR, ,               PSMode,           0, "1"
HKR, ,               PSControl, 0x00010001, 0x00000000

[DisablePSMode.reg]
HKR, ,               PSMode,           0, "0"

[MaxClientNum8.reg]
HKR, ,               MaxClientNum, 0x00010001, 0x00000008

[SingleBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
;HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
;HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
;HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
;HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
;HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
;HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
;HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

[DefaultBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
;HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
;HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
;HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
;HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
;HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
;HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
;HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; 5G Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
;HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
;HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
;HKR, NDI\params\CountryRegionABand,    default,            0, "0"
;HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
;HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
;HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
;HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
;HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
;HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
;HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
;HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
;HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
;HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
;HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%
;HKR, NDI\params\CountryRegionABand\enum,11,                0, %CountryRegion5G_11%
;HKR, NDI\params\CountryRegionABand\enum,12,                0, %CountryRegion5G_12%
;HKR, NDI\params\CountryRegionABand\enum,13,                0, %CountryRegion5G_13%
;HKR, NDI\params\CountryRegionABand\enum,14,                0, %CountryRegion5G_14%
;HKR, NDI\params\CountryRegionABand\enum,15,                0, %CountryRegion5G_15%
;HKR, NDI\params\CountryRegionABand\enum,16,                0, %CountryRegion5G_16%

[AdhocN.reg]
;
; AdhocNMode
;
HKR, ,                            AdhocNMode,      0, "0"
;HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
;HKR, NDI\params\AdhocNMode,       type,            0, "enum"
;HKR, NDI\params\AdhocNMode,       default,         0, "0"
;HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
;HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable%

;
; Customer Request
;
[LinkSpeedStatus.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "1"

[GainProSpeed.reg]
HKR, ,                            GainProSpeed, 0x00010001, 0x00000300 

[LinkSpeedControl.reg]
HKR, ,                            LinkSpeedControl, 0x00010001, 0x00000001 

; Customer request for Allied
[Customer1.reg]
; Vendor Description
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%
; WPS Device Name
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%

[Customer2.reg]
;
; D-Link Request
;
; WMMCapable
HKR, ,                            WMMCapable,      0, "1"
; Show Hidden SSID in Site Survey Page
HKR, ,                            ShowHiddenSSID,  0, "1"   ; 0=disable(default), 1=enable
; Enable TX Burst
HKR, ,                            TXBurst,         0, "1"
; DLSCapable
HKR, ,                            DLSCapable,      0, "1"

[FastRoaming.reg]
HKR, ,                                 FastRoamingSensitivity, 0, "2"
HKR, NDI\params\FastRoamingSensitivity,    ParamDesc,          0, %FAST_ROAMING_SENSITIVITY_STR%
HKR, NDI\params\FastRoamingSensitivity,    type,               0, "enum"
HKR, NDI\params\FastRoamingSensitivity,    default,            0, "2"
HKR, NDI\params\FastRoamingSensitivity\enum,1,                 0, %LOWEST_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,2,                 0, %MEDIUM_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,4,                 0, %HIGHEST_STR%

;
; Remove registry
;
[RegRemove.delReg]
; Remove CountryRegion
HKR, NDI\params\CountryRegion
HKR, NDI\params\CountryRegionABand

; Remove IEEE80211H
HKR, NDI\params\IEEE80211H
;
; RaCoInstaller Options
;
[CoInstOpt_DisableN.reg]
HKR, ,                    RaCoInstOpt,      0,"00001111"
HKR, ,                    CountryWirelessMode,     0x00010001, 0x00001000 

; WirelessMode
HKR, ,                            WirelessMode,    0, "3"

; CoInstaller Options , Enable 11n feature in Morocco, Russia, Ukraine.
[CoInstOpt_DLink.reg]
HKR, ,                            RaCoInstOpt,      0,"00001111"
; WirelessMode
HKR, ,                            WirelessMode,    0, "5"
; CountryWirelessMode
HKR, ,                            CountryWirelessMode,    0x10001, "0x11101110"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInstx.dll,ClassCoInstaller"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
CoInstaller.CopyFiles   = 11

[NT.CopyFiles]
Drt2860.sys                        ; NT Installation

[CoInstaller.CopyFiles]
RaCoInstx.dll
RaCoInst.dat

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
Drt2860.sys                = 1
RaCoInstx.dll             = 1
RaCoInst.dat              = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT80x86.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT80x86"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\DRT2860.sys
LoadOrderGroup              = NDIS


[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\DRT2860.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
D-Link                      = "D-Link Corporation"

;*******************************************************************************************
; Device description
;*******************************************************************************************

D-Link_3C04.DeviceDesc      = "D-Link DWA-525 Wireless N 150 Desktop Adapter"
D-Link_3C05.DeviceDesc      = "D-Link DWA-525 Wireless N 150 Desktop Adapter(rev.A2)"
D-Link_3C06.DeviceDesc      = "D-Link DWA-548 Wireless N PCIe Desktop Adapter"

INSTALL_DISK_STR            = "D-Link 802.11n Wireless LAN Installation Disk"

Generic.Service.DispName    = "D-Link 802.11n Wireless Driver"

; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
;SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "6"
WPS_DEVNAME_DEF_STR         = "D-Link Client"

RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Local MAC Network Address"
PSMode                      = "Power Saving Mode"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc support 802.11n"
WMMCapable                  = "WMM Capable"
APSDCapable                 = "APSD Capable"
APSDAC_BE                   = "AC_BE support APSD"
APSDAC_BK                   = "AC_BK support APSD"
APSDAC_VI                   = "AC_VI support APSD"
APSDAC_VO                   = "AC_VO support APSD"
FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensitivity"
LOWEST_STR                  = "Lowest"
MEDIUM_STR                  = "Medium"
HIGHEST_STR                 = "Highest"