==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For SUN PC-NFS V5.0 users
==================================================================
    (c) 1998 Copyright D-Link Corporation ALL RIGHTS RESERVED


This document contains DFE-650 Fast Ethernet PC Card installation notes,
which is not included in the DFE-650 Fast Ethernet PC Card USER'S GUIDE
or onscreen instructions, for SUN PC-NFS V5.0 users.



This document contains information on the following topics:

1.0   Overview
2.0   Installation Notes

---------------------------------------------------------------------

1.0 Overview
------------

SUN PC-NFS V5.0 users please also refer to the following:

     -------------------------------------------------------------------
        File            Description/Installation Notes
     -------------------------------------------------------------------

     INST_DOS.TXT       Overall Installation notes for DOS users,
                        including users of Windows 3.1/3.11.
     \NDIS2\README.TXT  Overall installation notes for all NDIS users


2.0   Installation Notes
------------------------

    Note: If a user would like to use an ODI MLID driver, please refer to
          the \NETWARE\PCNFS.TXT file.
          If a user would like to use an PACKET driver, please refer to
          the \PKTDRV\PCNFS.TXT file.

    2.1 Installation Notes for NDIS Driver

        When using PC-NFS concurrently with LAN Manager, select the
        NDIS option from the PC-NFS installation screen. This option
        works with the NDIS driver included in the provided driver
        diskette. Copy the files listed below into the \NFS directory
        of your hard disk.These files will be used in the installation.

        File              Description
        ------------     ----------------------------------------------
        NFS-NDIS.SYS      PC-NFS driver program
        DFE650.DOS         NDIS driver program
        PROTMAN.SYS       MS PROTOCOL MANAGER
        NETBIND.EXE       MS LAN MANAGER Netbind

        The following show some example configuration files:


                   *** Example CONFIG.SYS file  ***
            -------------------------------------------

       SWITCHES=/F
       DEVICE=C:\HIMEM.SYS
       DEVICE=C:\EMM386.EXE NOEMS X=D000-D7FF
       DOS=HIGH,UMB
       BUFFERS=10,0
       FILES=40
       STACKS=0,0
       LASTDRIVE=G
       SHELL=C:\DOS\COMMAND.COM C:\DOS /P
       DEVICE=C:\NFS\PCNFS.SYS /l40
       DEVICE=C:\NFS\SOCKDRV.SYS
       DEVICE=C:\LANMAN\PROTMAN.SYS /I:C:\LANMAN
       DEVICE=C:\LANMAN\NFS-NDIS.SYS
       DEVICE=C:\LANMAN\DFE650.DOS



                   *** Example AUTOEXEC.BAT file  ***
            -------------------------------------------

       SET TZ=EST5EDT
       C:\DOS\SMARTDRV.EXE
       @PROMPT $p$g
       PATH=C:\NFS;C:\DOS
       C:\LANMAN\NETBIND
       SET TEMP=C:\DOS
       SET NFSDRIVE=C
       SET NFSPATH=C:\NFS
       SET TN_DIR=C:\NFS\TELNET
       C:\NFS\PRT *
       C:\NFS\NET INIT


                  *** Example PROTOCOL.INI file  ***
            -------------------------------------------

       [PROTOCOL MANAGER]
             DriverName   = PROTMAN$

       [DFE650]
               DRIVERNAME = DFE650$
       [NFS-NDIS]
             DriverName   = NFSLINK$
             Bindings     = DFE650


        To use the NDIS driver, the user needs to obtain a PC-NFS 5.0
        QUIKNDIS diskette which will install all but the DFE-650 driver.

