==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For Banyan Vines Users
==================================================================
    (c) 1998 Copyright D-Link Corporation ALL RIGHTS RESERVED

This document contains DFE-650 Fast Ethernet PC Card installation notes,
which is not included in the DFE-650 Fast Ethernet PC Card USER'S GUIDE
or onscreen instructions, for Banyan users.


This document contains information on the following topics:

1.0   Overview
2.0   Installation Notes
___________________________________________________________________



1.0 Overview
------------

Banyan Vines users please also refer to the following:

-------------------------------------------------------------------
 File                Description/Installation Notes
-------------------------------------------------------------------

INST_DOS.TXT         Overall Installation notes for DOS users,
                     including users of Windows 3.1/3.11.
\NDIS2\README.TXT    Overall installation notes for all NDIS users


 2.0   Installation Notes
-------------------------
    There are two methods to copy  files from the Banyan VINES
    workstation to the bootable diskette or subdirectory on the hard
    disk.

    2.1  Method 1:
         Run INSTALL which is included in the diskette labeled
         "VINES MASTER DISK", then follow the given instructions to copy
         files.

    2.2  Method 2:
        1. Execute the 'BAN' command.

        2. Login to VINES system.

        3. Execute the 'PCCOPY' command.

        4. Select the 'NDIS Ethernet' option and follow the instructions
           for copying files.

        5. Insert the driver diskette in Drive A and the prepared
           bootable diskette in Drive B. Then, copy the appropriate NDIS
           driver file DFE650.DOS from Drive A to Drive B or to the
           subdirectory of the hard disk.

        6. Create a CONFIG.SYS file with the following statements:

           DEVICE=PROTMAN.DOS /I:A:\
           DEVICE=DFE650.DOS

           NOTE:
           A:\ is the path where Banyan VINES workstation files reside.

        7. Create a DFE650.NIF file containing the following statements:

           Model = D-Link DFE-650 Fast Ethernet PC Card
           Path = A:\
           DeviceDriver = DFE650.DOS
           DeviceName = DFE650$
           Type = NDIS

           NOTE:
           A:\ is the path where Banyan VINES workstation files reside.

        8. Create a PROTOCOL.INI file with the following lines:

           [PROTOCOL MANAGER]
           drivername = PROTMAN$

           [VINES_XIF]
           drivername = NDISBAN$
           bindings = "DFE650"

           [DFE650]
           drivername = DFE650$

        9. Execute the 'PCCONFIG' command.

           A "CONFIGURING A PC FOR THE NETWORK" message appears on the
           screen. The program then provides some options you can select.

       10. Select "1 - Network Card Settings".

           Another screen appears for selecting some options.

       11. Select "NDIS Ethernet".

       12. Select the appropriate configuration of the adapter.

       13. After configuring the adapter, you return to the main screen.
           Select "2 - Login Environment Settings".

       14. From the next screen, select "NDIS Ethernet".

           The 'PCCONFIG.DB' file will then be created.

       15. Restart your computer.

       16. Login to VINES by executing the 'BAN' command.
