[DFE650]
Type = NDIS
Title = "D-Link DFE-650 Fast Ethernet PC Card"
Version = 2.02
Drivername = DFE650$
Xports = NETBEUI LANDD

[FILE]
Name = DFE650.OS2
Path = IBMCOM\MACS

; Parameter start

[NETADDRESS]
tag = NETADDRESS
display = "Network adapter address"
type = Hexstring
Strlength = 12
optional = YES
editable = YES
help = "This parameter overrides the network address of the network
 adapter card.  The value of this parameter is a hexadecimal string of
 12 digits, as in 020001020304.  The address
 must be unique among all other network adapter addresses on the
 network."

[CONNECTION]
tag = CONNECTION
display = "Connection Type"
type = string
Strlength = 12
Set = AUTOSENSE, MB100_Half, MB10_Full, MB10_Half
default = AUTOSENSE
optional = YES
editable = YES
help = "This parameter specifies the connection type for the card.
 The valid connection type are AUTOSENSE, MB100_Half, MB10_Full,
 and MB10_Half. "


