==================================================================
NOTES ON
Installing D-Link DFE-650 Fast Ethernet PC Card
For WIN/TCP PathWay Access Users
==================================================================
    (c) 1998 Copyright D-Link Corporation  ALL RIGHTS RESERVED


This document contains DFE-650 Fast Ethernet PC Card installation notes,
which is not included in the DFE-650 Fast Ethernet PC Card USER'S GUIDE
or onscreen instructions, for WIN/TCP PathWay Access users.


This document contains information on the following topics:

1.0   Overview
2.0   Installation Notes

--------------------------------------------------------------------


1.0 Overview
------------

WIN/TCP Pathway users, please also refer to the following:

-------------------------------------------------------------------
File                Description/Installation Notes
-------------------------------------------------------------------
INST_DOS.TXT        Overall Installation notes for DOS users,
                    including users of Windows 3.1/3.11.
\NDIS2\README.TXT   Overall installation notes for all NDIS users


 2.0   Installation Notes
-------------------------

        1. Copy the DFE650.DOS file into your C:\LANMAN directory.

        2. Change to the C:\LANMAN directory, and create a
           PROTOCOL.INI text file with the following statements:

                [DFE650]
                drivername = DFE650$


        3. Add the following statements to your CONFIG.SYS file:
           device=c:\LANMAN\DFE650.DOS


        4. Add the following statements to your AUTOEXEC.BAT file:

                ndis
                winbind
                wintcp

        5. Restart your computer and WinTCP Pathways should be active.
